20ft Nedo Industrial Line Elevating Tripod 210710

**Features:**

* Indirect gear to easily lift and lower heavy instruments
* Reinforced gear unit for extra durability and less wear and tear
* Twist proof elevating column with centric clamp
* Tripod legs made of strong aluminum profiles and leg struts for extra stability

**Technical specifications:**

* Min. effective height approx. 1.12 m
* Max. effective height approx. 5.00 m
* Depth of shaft approx. 4.00 m
* Retracted length approx.1.21 m
* Holding screw: 5/8’’ thread
* Tripod adapter: 3/8’’ thread
* Weight approx. 8.9 kg
* Tripod plate flat, Ø 110 mm
* Tripod head and joints made of aluminium
* Use of the laser scanner above and below the elevating tripod
* mm graduation on telescopic tube
* Twist proof elevating column with centric clamp
* Suitable for shafts with a diameter of 205 cm

 